<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="77.47" width="0.3048" layer="20"/>
<wire x1="0" y1="77.47" x2="105.41" y2="77.47" width="0.3048" layer="20"/>
<wire x1="105.41" y1="77.47" x2="105.41" y2="3.81" width="0.3048" layer="20"/>
<wire x1="105.41" y1="3.81" x2="101.6" y2="0" width="0.3048" layer="20"/>
<wire x1="101.6" y1="0" x2="0" y2="0" width="0.3048" layer="20"/>
<text>Energy Monitor
Input Board v1.1</text>
<text>ngharo@gmail.com</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3528">
<description>Generic EIA 3528 polarized tantalum capacitor</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="arduino_due_shield">
<packages>
<package name="ARDUINO_DUE_SHIELD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="CT1" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="ARDUINO_DUE1" library="arduino_due_shield" package="ARDUINO_DUE_SHIELD" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT2" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT3" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT4" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT5" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT6" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT7" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT8" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT9" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT10" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08698"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="CT11" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="EIA3528" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="R1" pad="2"/>
<contactref element="CT1" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A0"/>
</signal>
<signal name="CT1_S">
<contactref element="R1" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="CT1" pad="SLEEVE"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="R12" pad="1"/>
<contactref element="C1" pad="C"/>
<contactref element="ARDUINO_DUE1" pad="GND_1"/>
<contactref element="ARDUINO_DUE1" pad="GND"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="C3" pad="C"/>
<contactref element="R9" pad="1"/>
<contactref element="C4" pad="C"/>
<contactref element="R14" pad="1"/>
<contactref element="C5" pad="C"/>
<contactref element="R17" pad="1"/>
<contactref element="C6" pad="C"/>
<contactref element="R20" pad="1"/>
<contactref element="C7" pad="C"/>
<contactref element="R23" pad="1"/>
<contactref element="C8" pad="C"/>
<contactref element="R26" pad="1"/>
<contactref element="C9" pad="C"/>
<contactref element="R29" pad="1"/>
<contactref element="C10" pad="C"/>
<contactref element="R32" pad="1"/>
<contactref element="C11" pad="C"/>
<contactref element="C12" pad="C"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="CT2_S">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="CT2" pad="SLEEVE"/>
<contactref element="C2" pad="A"/>
</signal>
<signal name="CT3_S">
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="CT3" pad="SLEEVE"/>
<contactref element="C3" pad="A"/>
</signal>
<signal name="CT4_S">
<contactref element="R8" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="CT4" pad="SLEEVE"/>
<contactref element="C4" pad="A"/>
</signal>
<signal name="CT5_S">
<contactref element="R11" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="CT5" pad="SLEEVE"/>
<contactref element="C5" pad="A"/>
</signal>
<signal name="CT6_S">
<contactref element="R16" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="CT6" pad="SLEEVE"/>
<contactref element="C6" pad="A"/>
</signal>
<signal name="CT7_S">
<contactref element="R19" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="CT7" pad="SLEEVE"/>
<contactref element="C7" pad="A"/>
</signal>
<signal name="A11">
<contactref element="ARDUINO_DUE1" pad="A11"/>
<contactref element="R35" pad="1"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="A1">
<contactref element="R2" pad="2"/>
<contactref element="CT2" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A1"/>
</signal>
<signal name="A2">
<contactref element="R5" pad="2"/>
<contactref element="CT3" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A2"/>
</signal>
<signal name="A3">
<contactref element="R8" pad="2"/>
<contactref element="CT4" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A3"/>
</signal>
<signal name="A4">
<contactref element="R11" pad="2"/>
<contactref element="CT5" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A4"/>
</signal>
<signal name="A5">
<contactref element="R16" pad="2"/>
<contactref element="CT6" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A5"/>
</signal>
<signal name="A6">
<contactref element="R19" pad="2"/>
<contactref element="CT7" pad="TIP"/>
<contactref element="ARDUINO_DUE1" pad="A6"/>
</signal>
<signal name="A7">
<contactref element="ARDUINO_DUE1" pad="A7"/>
<contactref element="R22" pad="2"/>
<contactref element="CT8" pad="TIP"/>
</signal>
<signal name="A8">
<contactref element="ARDUINO_DUE1" pad="A8"/>
<contactref element="R25" pad="2"/>
<contactref element="CT9" pad="TIP"/>
</signal>
<signal name="A9">
<contactref element="ARDUINO_DUE1" pad="A9"/>
<contactref element="R28" pad="2"/>
<contactref element="CT10" pad="TIP"/>
</signal>
<signal name="A10">
<contactref element="ARDUINO_DUE1" pad="A10"/>
<contactref element="R31" pad="2"/>
<contactref element="CT11" pad="TIP"/>
</signal>
<signal name="CT8_S">
<contactref element="R22" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="CT8" pad="SLEEVE"/>
<contactref element="C8" pad="A"/>
</signal>
<signal name="CT9_S">
<contactref element="R25" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="CT9" pad="SLEEVE"/>
<contactref element="C9" pad="A"/>
</signal>
<signal name="CT10_S">
<contactref element="R28" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="CT10" pad="SLEEVE"/>
<contactref element="C10" pad="A"/>
</signal>
<signal name="CT11_S">
<contactref element="R31" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="CT11" pad="SLEEVE"/>
<contactref element="C11" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R35" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="V_S">
<contactref element="R34" pad="1"/>
<contactref element="C12" pad="A"/>
<contactref element="R36" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="ARDUINO_DUE1" pad="5V0"/>
<contactref element="R13" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R36" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
